{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["加工说明书","Sheet2","Sheet3"],"not_rendered":{"images":1,"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"加工说明书","index":0,"n_rows":56,"n_cols":15,"rows_kept":56,"merged":[[0,0,0,15],[1,0,1,1],[1,2,1,4],[1,5,1,6],[1,7,1,8],[1,9,1,11],[1,12,1,15],[2,0,2,15],[3,0,5,11],[3,12,4,15],[5,12,5,13],[5,14,5,15],[6,1,6,3],[6,6,7,9],[6,10,6,12],[6,13,6,15],[7,1,7,3],[7,10,7,14],[8,1,8,3],[8,4,8,5],[9,1,9,15],[10,1,10,3],[10,7,10,8],[10,9,10,15],[11,1,11,3],[11,7,11,8],[11,9,11,15],[12,1,12,3],[12,10,12,11],[12,12,12,15],[13,1,13,3],[13,6,13,7],[13,10,13,11],[13,12,13,15],[14,1,14,3],[14,10,14,11],[14,12,14,15],[15,10,15,11],[15,12,15,15],[16,1,16,15],[17,1,17,3],[17,12,17,15],[18,1,18,5],[18,10,18,11],[18,12,18,15],[19,1,19,3],[19,7,19,8],[19,10,19,11],[20,1,20,3],[20,10,20,15],[22,1,22,3],[22,13,22,14],[23,1,23,3],[23,10,23,15],[26,1,26,3],[27,7,27,14],[29,1,29,15],[30,1,30,3],[30,6,30,11],[30,12,30,15],[31,1,31,3],[31,4,31,5],[31,6,31,11],[31,12,31,15],[32,1,32,3],[32,4,32,5],[32,6,32,11],[32,12,32,15],[33,1,33,3],[33,4,33,5],[33,6,33,11],[33,12,33,15],[34,1,34,3],[34,4,34,5],[34,6,34,11],[34,12,34,15],[35,1,35,3],[35,4,35,5],[35,6,35,11],[35,12,35,15],[36,1,36,3],[36,4,36,5],[36,6,36,11],[36,12,36,15],[37,1,37,3],[37,4,37,5],[37,6,37,11],[37,12,37,15],[38,1,38,3],[38,4,38,5],[38,6,38,11],[38,12,38,15],[39,1,39,3],[39,4,39,5],[39,6,39,11],[39,12,39,15],[40,1,40,3],[40,4,40,5],[40,6,40,11],[40,12,40,15],[41,1,41,3],[41,4,41,5],[41,6,41,11],[41,12,41,15],[42,1,42,3],[42,4,42,5],[42,6,42,11],[42,12,42,15],[43,0,43,2],[44,0,46,15],[47,0,47,15],[48,0,48,1],[48,2,48,7],[48,9,48,15],[49,0,49,1],[49,2,49,7],[49,9,49,15],[50,0,50,1],[50,2,50,7],[51,0,51,1],[51,2,51,7],[52,0,52,1],[52,2,52,7],[53,0,53,1],[53,2,53,7],[53,9,53,15],[54,0,54,1],[54,2,54,7],[54,9,54,15],[55,0,55,1],[55,2,55,7],[55,9,55,15],[56,9,56,15]],"flags":["formulas_cached_only"]}
["牧泰莱电路PCB加工工艺要求说明书"]
["文件名：",{"$nulls":4},"版本号：",{"$nulls":3},"物料名称："]
["PCB加工要求："]
[]
[]
[{"$nulls":12},"附图"]
[null,"1.数        量：",{"$nulls":3},"块",{"$nulls":4},"交货日期："]
[null,"2.层        数："]
[null,"3.尺        寸：",{"$nulls":4},"X",null,null,"mm","拼版尺寸",null,null,"X"]
[null,"备注：单只尺寸小于50mm*50mm或板边无焊接夹位的产品建议拼版加工，具体拼版方式见拼版确认函"]
[null,"4.板        厚：",{"$nulls":5},"其它："]
[null,"5.材        料：",{"$nulls":5},"其他材料："]
[null,"6.完成铜厚度：",null,null,"内层",null,null,"外层",null,null,"其它："]
[null,"7.阻        焊：",{"$nulls":4},"颜    色：",{"$nulls":3},"其它："]
[null,"8.字        符：",{"$nulls":4},"颜    色：",{"$nulls":3},"其它："]
[null,"9.过孔处理方式：",{"$nulls":8},"其它："]
[null,"注：BGA处默认塞孔，无需塞孔或其他方式请说明。"]
[null,"10.测        试："]
[null,"11.设计软件及其版本：",{"$nulls":8},"其它："]
[null,"12.金  手  指：",{"$nulls":3},"有","金厚",null,null,"UINCH","   倒角:",null,null,"度","深度"]
[null,"13.表面涂层：",{"$nulls":7},"其它："]
[null,"14.标记要求：",null,"厂商标记",null,null," ",null,null,"无铅标记：",null,null,"档案号："]
[null,"UL标记：",{"$nulls":7},"防静电："]
[null,"制作日期：",{"$nulls":7},"其它："]
[]
[null,"15.交货方式：",{"$nulls":5},"单元/片",null,"拼板交货允许报废",{"$nulls":4},"PCS/SET"]
[null,"16.交货随附资料："]
[]
[null,"17.   提供贴片钢网文件",{"$nulls":4},"提供生产Gerber文件",{"$nulls":4},"提供生产Gerber文件确认后再生产"]
[null,"18.叠层顺序与阻抗要求：以下叠层顺序是从顶层（TOP层）看"]
[null,"层次排列",null,null,"层的文件名",null,"控制阻抗的线宽/间距",{"$nulls":5},"阻抗要求及公差(ohm)"]
[null,"Top Layer："]
[null,"Layer   2："]
[null,"Layer   3："]
[null,"Layer   4："]
[null,"Layer   5："]
[null,"Layer   6："]
[null,"Layer   7："]
[null,"Layer   8："]
[null,"Layer   9："]
[null,"Layer   10："]
[null,"Layer   11："]
[null,"Bottom Layer："]
["其他特殊说明："]
[]
[]
[]
["以上说明若与提供文件内说明不一致时以此处说明为准!"]
["公司名称",{"$nulls":8},"牧泰莱电路技术有限公司"]
["部        门：",null,"合同联系人"]
["联系人1：",{"$nulls":8},"电话：","0731-82786288"]
["电        话："]
["邮        箱：",{"$nulls":8},"收件专用邮箱： ",null,null,"text@mtlpcb.com"]
["联系人2：",null,"技术联系人",{"$nulls":6},"文件初审工程师："]
["电        话：",{"$nulls":8},"公司网址：www.mtlpcb.com"]
["邮        箱："]

{"sheet":"Sheet2","index":1,"n_rows":24,"n_cols":15,"rows_kept":24,"flags":["formulas_cached_only"]}
["无"]
["1张","单面","0.2mm","H/H oz","H/H oz","单面顶层","绿色","白色","Gerber 文件","FR-4",null,"年周","无铅标记","有铅喷锡","覆盖"]
["2张","双面","0.3mm","1/1 oz","1/1 oz","单面底层","红色","黑色","PADS  2005","FR-4 IT-180A",null,"周年","防静电","无铅喷锡","不覆盖"]
["3张","三层","0.4mm","2/2 oz","1.5/1.5 oz","双面印刷","蓝色","黄色","PADS  2005SP2","Rogers 4003",null,"年月日",null,"化学沉金","部分覆盖"]
["4张","四层","0.5mm","3/3 oz","2/2 oz","无","黑色","红色","PADS  2007","Rogers 4350",null,"日月年",null,"OSP(防氧化）","部分塞孔"]
["5张","五层","0.6mm","4/4 oz","3/3 oz",null,"白色","其它规格","PADS  2009","Ro 其它型号",null,"其它",null,"沉锡","覆盖不塞"]
["6张","六层","0.7mm","5/5 oz","4/4 oz",null,"哑光绿色",null,"Protel 98","Taconic系列",{"$nulls":3},"沉银","覆盖塞孔"]
["7张","七层","0.8mm","6/6 oz","5/5 oz",null,"哑光黑色",null,"Protel 99SE","铝基材料",{"$nulls":3},"其它","根据文件"]
["8张","八层","0.9mm","其它规格","6/6 oz",null,"哑光蓝色",null,"Protel DXP 2004","RF-35",{"$nulls":4},"其它"]
[null,"九层","1.0mm",null,"其它规格",null,"其它规格",null,"Altium Designer 6.9","Arlon"]
[null,"十层","1.1mm",{"$nulls":5},"Altium Designer 10","其它"]
[null,"十二层","1.2mm",{"$nulls":5},"PowerPCB 2.1"]
[null,"十四层","1.3mm",{"$nulls":5},"PowerPCB 4.0"]
[null,"十六层","1.5mm",{"$nulls":5},"PowerPCB 5.0"]
[null,"十八层","1.6mm",{"$nulls":5},"其它格式"]
[null,"二十层","1.8mm"]
[null,"二十四层","2.0mm"]
[null,"其它","2.4mm"]
[null,null,"2.5mm"]
[null,null,"3.0mm"]
[null,null,"4.0mm"]
[null,null,"5.0mm"]
[null,null,"6.0mm"]
[null,null,"其它规格"]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}